
 STMicroelectronics
=================================================================

1, 71xboot-R10.bin		
--STR710-EVAL bootloader: The bootloader image
It has to be programmed in the beginning of external flash
memory (0x60000000) and get executed first after power up or reset.
It allows loading image into the external SRAM (0x62000000) through 
a serial port.

2, zimage.bin			
--uClinux image file which should be programmed to 64K offset of the 
external flash.(zimage file with user applications built in) 

4, jffs2.img
--JFFS2 data storage image with an I2C EEPROM programmer included. 
This file should be programmed  to 2M offset of the external flash.
