/**
  @page EEPROM_Emulation AN2594 EEPROM_Emulation Readme file
  
  @verbatim
  ******************** (C) COPYRIGHT 2009 STMicroelectronics *******************
  * @file     EEPROM_Emulation/readme.txt 
  * @author   MCD Application Team
  * @version  V3.1.0
  * @date     07/27/2009
  * @brief    Description of the AN2594 "EEPROM emulation in STM32F10x microcontrollers".
  ******************************************************************************
  * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
  * TIME. AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY
  * DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING
  * FROM THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
  ******************************************************************************
   @endverbatim

@par Example Description 

This AN describes a software method for emulating EEPROM using the onchip Flash
memory of the STM32F10xx  devices.

@par Directory contents 

+ inc 
  - EEPROM_Emulation/inc/stm32f10x_conf.h     Library Configuration file
  - EEPROM_Emulation/inc/stm32f10x_it.h       Interrupt handlers header file
  - EEPROM_Emulation/inc/eeprom.h             EEPROM emulation Header file

+ src 
  - EEPROM_Emulation/src/stm32f10x_it.c    Interrupt handlers
  - EEPROM_Emulation/src/eeprom.c          EEPROM emulation firmware functions
  - EEPROM_Emulation/src/main.c            Main program  


@par Hardware and Software environment 

  - This example runs on STM32F10x Connectivity line, High-Density, Medium-Density 
    and Low-Density Devices.
  
  - This example has been tested with STMicroelectronics STM3210C-EVAL (STM32F10x 
    Connectivity line), STM3210E-EVAL (STM32F10x High-Density) and STM3210B-EVAL
    (STM32F10x Medium-Density) evaluation boards and can be easily tailored to
    any other supported device and development board.


@par How to use it ?  

 - RVMDK 
    - Open the EEPROM_Emulation.Uv2 project
    - In the build toolbar select the project config:
        - STM3210C-EVAL: to configure the project for STM32 Connectivity line devices
        - STM3210B-EVAL: to configure the project for STM32 Medium-density devices
        - STM3210E-EVAL: to configure the project for STM32 High-density devices
    - Rebuild all files: Project->Rebuild all target files
    - Load project image: Debug->Start/Stop Debug Session
    - Run program: Debug->Run (F5)    

 - EWARMv5 (v5.30) 
    - Open the EEPROM_Emulation.eww workspace.
    - In the workspace toolbar select the project config:
        - STM3210C-EVAL: to configure the project for STM32 Connectivity line devices
        - STM3210B-EVAL: to configure the project for STM32 Medium-density devices
        - STM3210E-EVAL: to configure the project for STM32 High-density devices
    - Rebuild all files: Project->Rebuild all
    - Load project image: Project->Debug
    - Run program: Debug->Go(F5)

 - RIDE 
    - Open the EEPROM_Emulation.rprj project.
    - In the configuration toolbar(Project->properties) select the project config:
        - STM3210C-EVAL: to configure the project for STM32 Connectivity line devices
       - STM3210B-EVAL: to configure the project for STM32 Medium-density devices
       - STM3210E-EVAL: to configure the project for STM32 High-density devices
    - Rebuild all files: Project->build project
    - Load project image: Debug->start(ctrl+D)
    - Run program: Debug->Run(ctrl+F9)  

@note
 - Low-density devices are STM32F101xx and STM32F103xx microcontrollers where
   the Flash memory density ranges between 16 and 32 Kbytes.
 - Medium-density devices are STM32F101xx and STM32F103xx microcontrollers where
   the Flash memory density ranges between 32 and 128 Kbytes.
 - High-density devices are STM32F101xx and STM32F103xx microcontrollers where
   the Flash memory density ranges between 256 and 512 Kbytes.
 - Connectivity line devices are STM32F105xx and STM32F107xx microcontrollers.                

 * <h2><center>&copy; COPYRIGHT 2009 STMicroelectronics</center></h2>
 */
