# Release Notes for AN2598 "Smartcard interface with the STM32F10x microcontrollers" firmware Copyright 2009 STMicroelectronics
## Contents AN2598 "Smartcard interface with the STM32F10x microcontrollers" firmware update History License ## AN2598 "Smartcard interface with the STM32F10x microcontrollers" firmware update History ### V3.1.0 - 07/27/2009 Update to support the STM32F10x Connectivity Line devices. Add new workspace STM3210C-EVAL for EWARM, RIDE and RVMDK preconfigured projects Update with STM32F10x Standard Peripherals Library V3.1.0 CMSIS: system_stm32f10x.c file updated to fix bug in SetSysClockTo56() function (Flash wait state set to 1 instead of 2) ### V3.0.0 - 04/27/2009 AN2598 "Smartcard interface with the STM32F101xx and STM32F103xx" firmware updated with STM32F10x Standard Peripherals Library (StdPeriph_Lib) V3.0.0 AN2598 "Smartcard interface with the STM32F101xx and STM32F103xx" firmware is full CMSIS compliant STM32F10x Standard Peripherals Library Structure is updated. AN2598 "Smartcard interface with the STM32F101xx and STM32F103xx" firmware Package Architecture is enhanced For more details, please refer to AN2953 "How to migrate from the STM32F10xxx firmware library V2.0.3 to the STM32F10xxx standard peripheral library V3.0.0". ### V2.0.2 - 07/11/2008 Update according to USART driver update in FWLib V2.0.2 ### V2.0.1 - 06/13/2008 Remove the Firmware License Agreement file Update the source files's header to remove reference to the License ### V2.0 - 05/30/2008 Update with STM32F10x FWLib V2.0 to support the extra peripherals and features embedded in the STM32 High-density devices. Add support of STMicroelectronics STM3210E-EVAL evaluation board (in addition to STM3210B-EVAL) Add Firmware License Agreement file For more details about this example implementation, please refer to the AN2598 "Smartcard interface with the STM32F101xx and STM32F103xx", available for download from the ST microcontrollers website: www.st.com/stm32 Glossary Medium-density devices are STM32F101xx and STM32F103xx microcontrollers where the Flash memory density ranges between 32 and 128 Kbytes. High-density devices are STM32F101xx and STM32F103xx microcontrollers where the Flash memory density ranges between 256 and 512 Kbytes. ### V1.0 - 10/08/2007 Updated with STM32F10x FWLib V1.0 Add project with RIDE toolchain main.c Add "Delay" function with SysTick used as time base smartcard.c "SC_PTSConfig" and "SC_SendData" functions updated stm32f10x_it.c "USART3_IRQHandler" ISR updated ### V0.1 - 07/23/2007 Created. ## License The enclosed firmware and all the related documentation are not covered by a License Agreement, if you need such License you can contact your local STMicroelectronics office. THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME. AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS. For Complete on STM32(CORTEX M3) 32-Bit Microcontrollers visit www.st.com/STM32