                    FEBRUARY 18, 2003

     TO:   PC FABRICATOR

     FROM: KENDALL KELSEN AT WJ COMMUNICATION.

     RE:   FABRICATION OF PCB 452525PC REV 2
                          A/W 452525AW REV 2

    
     HERE ARE THE FILES THAT ARE REQUIRED FOR THE
     FABRICATION OF WJ COMMUNICATIONS PRINTED CIRCUIT BOARD.
     IF YOU HAVE ANY QUESTIONS PLEASE CONTACT Kendall Kelsen
     AT 408-577-6284 OR E-MAIL AT kendall.kelsen@WJ.COM 


     NO. LAYERS          : 4

     FILE NAME           CONTENTS
     L1.PHO              : LAYER 1 - COMPONENT SIDE
     L2.PHO              : LAYER 2 - GND PLANE
     L3.PHO              : LAYER 3 - GND PLANE
     L4.PHO              : LAYER 4 - BOTTOM SIDE
     
     SLLKT.PHO           : SILKSCREEN TOP (ANY REFERENCE 
                           DESIGNATORS LOCATED INSIDE THE COMPONENT 
                           BODY CAN BE REMOVED)

                             
     DM.PHO              : DRILL MASTER
     SMASKT.PHO          : SOLDERMASK TOP
          

     *.REP               : INDIVIDUAL APERTURE LIST FILES
                           FOR THE ABOVE GERBER FILES
     452525AW.REP        : COMBINED APERTURE REPORT

     
     DRL01.DRL           : EXCELLON DRILL FILE, EXCELLON
			   ASCII FORMAT
     DRL01.LST           : EXCELLON DRILL LIST, GENERIC
			   ASCII FORMAT
     DRL01.REP           : DRILL TOOL REPORT, ASCII FORMAT


     452525PC.PLT        : SHEET 1, FABRICATION DRAWING, HP MASTER
     
     Notes:
           1) On silkscreen layer, it's OK to use 6 mils lines where
              5 mils lines are.

	  
     

     

                 ================================

    